193-4Z-06K Sentrol 193 GuardSwitch Series Non-Contact Interlock/Position Switch, IP67, -40 to 180 F temp range, seamless 304 stainless steel, 120AC/28DC op voltage, 3A, 100VA/84W, SPDT, 6 ft lead.

* **Manufacturer:** Sentrol
* **Product Type:** Non-Contact Interlock/Position Switches
* **Product Family:** 193 GuardSwitch Series

**Product Description**

193-4Z-06K The 191/193 Series Seamless Stainless Steel GuardSwitch is a seamless stainless steel interlock/position sensor ideal for use in severe wash-down or chemical environments, such as food processing applications.  
  
**APPLICATIONS**

* USDA approved
* Food Processing Machines
* Chemical Industry Machinery
* Wash-down Environments

